02/10/02	V3.0i	EJZ
	Fixed uploading problem with little boxes. Would cause fault when attempting first channel.

02/11/02	V3.0j	EJZ
	If distance calculated from ended before all other RPM channels, the program would hang
		in an infinite loop.

02/18/02	V3.0k	EJZ
	Loading 'Car Setup' files would corrupt the configuration lists if 'Replace' mode was
		selected. The program would crash!

02/21/02	V3.0L	EJZ
	When loading a 'Car Setup', the new configuration would be accepted if the new config
		had more channels than the old config.

03/05/02	V3.0M	EJZ
	Edge Boxes with Firmware version 2.24 or higher, now supports uploading at 38.4K Baud.
	When loading Default Analog settings from '.ini' file, negative values were being
		reset to zero.
	RPM Channels were NOT setting all parameters from 'Default' settings.
	If 'Rear Wheel' definition existed in 'Default' settings, it was NOT being copied to
		the 'Uploaded' dataset.
	In 'Configure Data Logger', if Engine Type selected for RPM channels 2-5, PPR was NOT
		being updated correctly.
	If 'Single Cyl, 1/2 PPR' selected for RPM channels 2-5, the PPR value would be set
		to zero. This would cause MAJOR problems in Edge box.

04/03/02	V3.0N	EJZ
	Selecting ET-Slip Report could cause the program to crash if too many Digital Timer
		input events existed.
	Still had a problem uploading at 38.4K if any timers were turned on. The box would
		go back to 9600 after uploading each timer input.
	When entering ET-Slip data, if there was more than a few digital inputs, the program
		would crash.

07/19/02	V3.0P	EJZ
	When overlaying files, if file being overlayed did NOT contain same RPM channels,
		the program would crash.

08/01/02	V3.0Q	EJZ
	When reading ".TAC" files with Rear Wheel MPH saved in the file, the MPH would NOT
		be read correctly.
	When reading ".TAC" files with Analog Data, if Edit->Split-into-Laps was performed,
		the program would crash.
	When reading ".TBC" files made by V2.5A or V2.5B, the program would crash.

07/30/02	V3.1a	EJZ
	Changed Marker View to display Distance only if calculated.
	Changed Marker View to show Distance or Time for each Lap Viewed.
	User now has full color control for the 'Graph' and 'Track Map'.
	Allow user to turn on and off Analog scales.
	Revamped entire Menu Command structure.
	Channel Name column in Marker View will only appear if no markers have been set.
		After a marker has been set, column will toggle between Visible and All channels.
	When setting "Zero-Time", this would only work properly for Keyboard entry or if
		"Zero-Time" was equal to zero.
	Digital Inputs were always being set to display based on the type of input, not what
		the user desired.
	"Report->ET-Slip" will now turn on markers when using "Apply" or "OK" to exit.
	"Report->Lap Times" does NOT show mode for "Update Elapsed Time" check box when opened.
	In Color Menu; RPM, Analog, etc. All On/Off buttons effect only the selected session.
	In Color Menu; A button has been added to change the color for all the channels in a session.

08/05/02	V3.1b	EJZ
	Fixed problems with Lap Report Dialog. If any Pop-Up Dialog would occur while changing
		the Lap Times, the Lap Times would be reloaded from the original list. Why this
		was occurring, could produce other problems while editing Lap Times.
	Fixed problem with Move Lap Marker, it would only allow the first Session to be changed.

09/12/02	V3.1c	EJZ
	Fixed problem with "Edit->Data Alignment". It no longer causes the program to crash.
	Fixed problem with displaying one loaded session as MPH and the others as RPM.
	The Pulse per Rev settings for the RPM channels will now override the settings
		being upload from the data loggers.
	When uploading data, the Gear Ratio settings in the Default Transmission settings were
		not always being set correctly. This has been corrected.

09/18/02	V3.1d	EJZ
	Fixed problem with Data files not having any leading data before a Lap Marker. This
		cause some features NOT to work in Lap View Mode.
	The Marker View window now maintains a fixed width as the overall window size is changed.
	The program now remembers the last size of the Marker View window. Whichever window was
		closed last, this window will determine the size of the Marker View window for the
		next file opened.

09/19/02	V3.1e	EJZ
	Display "Top Half" mode was NOT being allowed for Analog Inputs. It always changed back to
		what the previous Display mode was.

10/02/02	V3.1f	EJZ
	Changed Lap color sequence for Lap View mode when setting all channels in a lap to a single
		color.
	Fixed the Start and Stop markers when changing to a dark background color. The markers would
		swap colors for both the Graph and Track Map.

10/07/02	V3.1g	EJZ
	When loading a file, the Marker View can now be set to the Right or Bottom of the Graph.
	You can now set the Green and Red Markers by clicking on the Track Map.

10/12/02	V3.1h	EJZ
	When Overlaying a file and the current file loaded was using Time-Offset, the current
		file would no longer be displayed using the Time-Offset value.
	When closing a file, the setting of the Marker View was being changed to how that
		file had the Marker View displayed.
	When no times where avaiable for ET-Slip report, the program would crash when activated.

10/29/02	V3.1j	EJZ
	When uploading data, if PPR is different from the box, the value is changed but
		the graph still reflects the box's value.
	If user double clicked Left or Right mouse button in Track Map View and no map had
		been drawn yet, the program would crash.
	On the inital opening of the Track Map View, the user will be prompted for the Lap
		to use to draw the map.
	Opening a file with Windows Explorer now works correctly.

11/02/02	V3.1k	EJZ
	If markers are not turned on, when double clicking on Track Map, the markers
		were not displayed for the graph and the Marker view was not updated.
	Misc. problems with the Left and Right Arrow keys not working correctly.
	If no starting Lap marker, the Track Map markers would not displaying correctly.
	Histogram time selection was not correct for data files that did not have data
		before the first Lap Marker or after the last Lap Marker.

11/20/02	V3.1m	EJZ
	Changed "SendMessage" to "PushMessage" to try and fix problem with the markers NOT being
		redrawn correctly when clearing Pop-Up menus from automaticly asking user for Track-Map
		lap number.

11/26/02	V3.2a	EJZ
	When Config List was being read from "INI" file, the "Active Settings" value was being
		limited to a value of 4 instead of 255. This was losing which configuration was the
		active configuration.
	When calculating amount of recording time for the large systems, it was NOT calculating the
		number of bytes used by Timers correctly.
	The capabililty to view Real-Time/Live Data from the large systems has been added. You will
		need at least V2.32 of the firmware for the Data Logger. The only restriction at this time
		is that this is NOT allowed while the Data Logger is recording data.
	The large systems can now record Input Battery voltage.  You will need at least "V2.32 w/ Battery"
		of the firmware for the Data Logger.
	When configuring Channel 17 thru 20 for the large systems, you will be restricted to the type
		of channel that this can be.
	You now can update the Firmware on the Data Logger from the
		"Settings->Update Firmware on Data Logger" menu.
	The background color for the Marker-View is now displayed as the same color as the Graph-View.
	It is now possible to Change/Zero analog offsets via the Green or Red Markers. This is accomplished
		via "Change Graph->Analog Channels->Change/Zero Analog Offset via Green/Red Marker".
	An interface has been added to dynamically link to Performance Trends 3D Suspension Analyzer program.
		This can be found under the "Tools" menu. For more information, contact your vendor.
	Print and Print-Previewing now allows you to Print/PreView the Marker Information. You can change the
		format; from View Channels to All Channels, etc., without effecting the way the Marker Info is being
		viewed on the screen.
	If view data was in "Lap Mode", access to the RPM/MPH, Analog and Digital Configuration menus were not
		always accessible.
	If the RPM/MPH channel being used for calculating distance traveled was not being displayed, switching
		between Distance and Time mode for X Axis could cause the graph to be drawn incorrectly.

01/21/03	V3.2b
	Added capability to view Left/Right and Front/Rear Accelerometers as a Friction Circle.
	Distances for a Dataset are now normalized. This forces all distances to be the same when viewing
		the X Axis as distance.

04/08/03	V3.2c
	Added two Drop Selections to the Tool Bar. The first is to select which file/session to view. The second
		is to select which window for the selected session to view.
	You can now change between having the Marker View on the right or bottom after the file has been loaded.
	The Friction Circle view now allows displaying of the L-R, F-R and Max G values for both markers.
	For 4-Channel systems, when the default view for an Analog channel was something other than "Full Scale",
		after uploading the scales would be wrong and the only way to view the data was "Full Scale".
	For 4-Channel systems, Analog channels of type "Customer Defined", "Pressure Transducer" and "VDO Pressure"
		would NOT display the correct value of the Green and Red markers in the Marker view.

04/29/03	V3.2d
	There is now an Export File option. It will export the data in an ASCII file for use in Excel, etc.
		The feature allows user to select which channels to export and at what sample rate.
	Changed appropriate Analog channels to reflect user selection of Imperial or Metric units.
	Fixed problems with Live Data with respect to the Misc. Analog Page.
	When adding a file for overlay, if file had been saved after "Viewed Lap Mode", it would cause the program
		to crash.

05/02/03	V3.2e
	Fixed Steering input for Live Data.

05/06/03	V3.2f
	When Overlaying files, the Data set name was not being updated to include the new file.
	If Battery Voltage input existed and the Spike Filter dialog was entered, the program would crash.
	Fixed the displaying of "Customer Defined" for Live Data.

06/05/03	V3.2g
	If changing the Accel inputs and they where not originally identified as "Left-Right" or "Front-Rear",
		the program would crash.
	If Dataset had been viewed in Lap Mode, calibrating the Analog channels from the markers would not
		change the calibration.
	This version is required in order to use Firmware V2.39 or later for the large Data Loggers.
	When changing an Analog type in the Configuration Dialog from/to T/C, the scan rate list was
		not being updated.
	When configuring Data Logger RPM channels, if you selected a different channel number, the program
		would crash. This has been resolved.
	When using "Live Data" to calibrate the Steering Wheel channel, the "Min" and "Max" values will now
		be a negative and a positive value instead of zero and a positive value.
	When using "Live Data" to calibrate the Steering Wheel and Throttle channels, they will now detect if
		the channel needs to be inverted.
	When loading a "Car File" in either RPM, Analog or Digital Settings, the new values for the Analog and
		Digital channels where not always being updated correctly for the display.

07/18/03	V3.2h
	When Exporting a file, if distance is being used for the X Axis, this will now be reported in the output
		file along with the time stamp.
	If trying to delete data using "Edit/Delete Data" and ET-Slip data has been entered, the program would
		crash. This has been resolved.
	If distance was calculated after setting the Green or Red marker, the distance for the marker would be
		displayed as "N/A".
	When adding a file for overlaying and distance has been calculated for the current file(s),
		many little problems with the Marker view would result.
	When Exporting data, ET-Slip data showed up as Lap Times.
	If wanting to use Engine RPM to calculate distance traveled and no rear tire definition
		existed, you were not allowed to add the rear tire definition.
	In RPM Setup, the Tire Diameter and Circumference now displays if expecting inches or centimeter.
	If entering the Lap Report with ET-Slip data, if user chooses to cancel, the program goes into a
		infinite loop until it crashes. The program no longer crashes but does enter the menu anyway.
	On Windows XP and 2000 operating systems, the program would crash when changing the RPM Channel
		number when configuring the channels for the larger data loggers.

07/25/03	V3.2j
	On Windows XP and 2000 operating systems, the program would crash when trying to add a new channel
		in the Digital Configuration menu.
	Added Interval times for the ET-Slip report.

10/07/03	V3.2k
	When drawing Track Map with a Drive Shaft mounted sensor, the program would crash. This was being
		caused by the tire size being defined with "Rear Wheel definition".
	When using the "Zero Analog Offset" feature with frequency based analogs, these channels were
		not being included in the list of choices.
	The "Traction Circle" was not checking to make sure that the Accels existed properly and would
		cause the program to crash if entered.
	When calibrating the "Steering" sensor with "Live Data", the "Zero" position was not being
		calculated correctly.
	When viewing the data in lap mode, the distance for each lap is normalized.
	Zooming on the Track Map is now supported. Zooming with the mouse is the same as with the Graph.
	If Com Port 5 thru 8 was being used, next time the program was restarted, Com Port 1 would be selected.
	Double clicking on the "Upload" tool bar icon would cause a "Com Port Already Open" error.
		This has been resolved.

10/08/03	V3.2m
	The capability to "Race" two or more laps against each other is now supported.

04/12/04	V3.2n
	When adding changes for GPS support, an error was introduced when uploading Timers that caused them
		to report erronous timer values.

06/21/04	V3.2p
	Fixed scroll bar problems with zooming on the Track Map.
	Fixed Restart Race Mode so that the Markers on the Graph and Track Map reset properly.
	Added "Auto-Scrolling" to the Track Map so that it follows the Race Mode markers.
	Fixed problems when viewing in "Metric" mode. Distances are now displayed in meters and Track Mapping
		will now work correctly.
	When reading in a file that was saved while in "Metric" mode, the tire sizes will not read correctly.
		Fix the tires sizes, resave the file and this will no longer happen.
	Digital Channels are now reported in the Marker View if it is not a verticle marker.
	When setting the Engine RPM channel to "Single Cyl, 4 cycle, 1/2 PPR", the RPMs would not always be
		reported correctly. Most the time it would appear at 1/2 the actual RPM.

08/26/04	V3.2q
	When using "Metric" mode, the Default settings were NOT be altered to reflect the change.
	Added user option to allow "Auto-Scrolling" on either the Green or Red marker for the Track Map.
	Fixed Scroll Bar problem on Graph when user would select the Scroll Bar Marker.
	Fixed importing a Car File so that it now works in all of the Setup Menus.
	In Digital Config, if the input is a Vertical Marker, "Invert" selection is grayed out.
	When a Digital Input is changed to a Lap Timer input, it will be moved to the Special Lap Timer Channel
		or it will have to be changed to something else.

09/01/2004	V3.2r
	Fixed some more problems with "Metric" mode with respect to distance calculations.
	Fixed problems with scrolling the Track Map when using the Scroll Position marker.

11/19/2004	V3.2s
	Fixed a problem with overlaying data files that caused the program to crash.
	Fixed the problem when changing the number of recording segments that caused the program to crash.
	Further enhancements to perfect the printing of the marker information.

11/26/2004	V3.3a
	Printing when distance is being viewed now prints correctly, end of data is not clipped.
	Added capability to "segment" the track map and produce a report.
	Added printing for Lap Segment Reports.
	Printing of Marker View has been improved.
	Fix problem with changing number of recording segment. The program no longer crashes.

4/27/2005	V3.3c
	Fixed problem of having more than 3 accelerometers for Live Data.
	Changed Configuration Menu to use "Tabbed" folders.
	Added Auto-Start and Controlled Outputs.
	Fixed RPM Defaults to override settings, no matter what, on Uploading if RPM Type is set to User-Defined.

5/13/2005	V3.3d
	When trying to delete data using the Green and/or Red marker(s) and a Zero Time offset has been set, the program
		might crash or not delete correctly.

7/07/2005	V3.3e
	Fixed a problem with changing display settings for Digital Inputs.
	Made changes to the communications protocal to improve use with USB Converters.
	Fixed problem with Pressure Sensors and Output Control.
